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FICTITIOUS DEMONSTRATION SAMPLE
RFQ SPE7L0-26-R-DEM4 (FICTITIOUS SOLICITATION)
	FICTIONAL DEMONSTRATION SAMPLE. DLA did not issue this solicitation. Every identifier, company, item, quantity, instruction, and date below is invented.


Header
Solicitation: SPE7L0-26-R-DEM4
Buying activity: DLA Land and Maritime (fictitious sample)
Issue date: 2026-07-01
Original return deadline: 2026-07-24 at 3:00 p.m. Eastern
Submission: enter quote fields in the DIBBS web quote form and upload the document package as one combined PDF using the DIBBS offer-upload link attached to this solicitation
Evaluation: manual review of price, delivery, responsibility, exact-product compliance, and the required document package
Master terms: DLA Master Solicitation for Automated Simplified Acquisitions, Revision 104, incorporated by reference for this fictional sample
The document-upload requirement comes from these solicitation instructions. The letter in the ninth position of the sample solicitation number does not create the requirement.
Line item 0001
NSN: 4820-01-DEM-0755
Item: check valve, hydraulic, poppet type, 3/4 inch, 3000 psi
Approved product: Calder Fluid Systems Corp, CAGE 0DEM7, part number CFS-2205-7, drawing CFS-2205 revision C
AMC/AMSC: 1D
Quantity and unit: 150 EA
Quantity variance: none
Requested delivery: 45 days after receipt of order
FOB: destination
Inspection and acceptance: origin unless the cognizant Contract Administration Office authorizes use of a Certificate of Conformance in writing after award; otherwise inspection and acceptance occur as directed by the award
Higher-level quality: ISO 9001:2015
Traceability: procurement note C03 and STO RQ018 apply
Export control: RQ032 not cited
Surplus: not solicited
Hazardous material: none
NAICS: 332912; size standard 1,000 employees
Exact packaging and marking data
The offeror shall include the full cost of the following packaging in its unit price and answer "Yes" to Meets Packaging Requirement only if it can comply:
Preservation method: MIL-STD-2073-1E Method 50
Unit pack quantity: 1 EA
Ports: keep the manufacturer's protective caps installed
Barrier: greaseproof and waterproof barrier around each capped valve
Cushioning: closed-cell cushioning fitted to prevent movement inside the unit container
Unit container: fiberboard box meeting ASTM D5118
Intermediate quantity: 10 unit packs per intermediate container
Exterior container: fiberboard shipping container meeting ASTM D5118, palletized when the shipment quantity requires it
Marking: MIL-STD-129R, including solicitation or award number, NSN, part number, approved-manufacturer CAGE, quantity and unit, and lot CFS-L2606-118
Web quote-form fields
Enter Bid Without Exception (BI) only if the offered product and every term above can be met without qualification. Enter the unit price, delivery days, quote-valid period, FOB, inspection point, Meets Packaging Requirement, ISO 9001:2015 quality answer, dealer status, actual manufacturing source, country of origin, and the applicable representations. Identify Calder Fluid Systems Corp, CAGE 0DEM7, as the actual manufacturing source. Do not describe Ardent Flow Distribution LLC as the manufacturer.
Required combined PDF, in this exact order
The combined PDF shall contain six tabs. Each tab shall state the solicitation number, NSN, approved-manufacturer CAGE, part number, offered lot, and quantity where applicable.
1. Cover and index with the offeror's UEI and CAGE.
1. Unsigned post-award Certificate of Conformance specimen. The specimen shall reproduce the certificate language in FAR 52.246-15(d). The offeror shall not date or sign it before award. Shipment under a Certificate of Conformance may occur only after written authorization from the cognizant Contract Administration Office.
1. Supply-chain traceability statement identifying every intermediary by name, location, and CAGE, with the documents that connect each link to the approved manufacturer.
1. Manufacturer and quality records for lot CFS-L2606-118: Calder Certificate of Conformance, certified material test report, proof-pressure report, seat-leakage report, incoming inspection record, and current ISO 9001:2015 evidence.
1. Packaging and marking compliance statement that repeats the exact packaging data above and identifies the packaging evidence used to support the price.
1. Technical-data and drawing-status statement confirming Calder part number CFS-2205-7 at drawing CFS-2205 revision C.
The six tabs shall be searchable, portrait-oriented, and combined into one PDF. File name: 8DEM2_SPE7L026RDEM4_DOCUMENT_PACKAGE.pdf. Do not password-protect the file.
Certificate text required in tab 2
The specimen shall reproduce this FAR 52.246-15(d) certificate text:
"I certify that on ______ [insert date], the ____ [insert Contractor's name] furnished the supplies or services called for by Contract No._____ via ____ [Carrier] on ________ [identify the bill of lading or shipping document] in accordance with all applicable requirements. I further certify that the supplies or services are of the quality specified and conform in all respects with the contract requirements, including specifications, drawings, preservation, packaging, packing, marking requirements, and physical item identification (part number), and are in the quantity shown on this or on the attached acceptance document."
The executed certificate shall include Date of Execution, Signature, and Title. The quotation package contains an unsigned specimen only.
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