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FICTITIOUS DEMONSTRATION SAMPLE
Tab 5: Packaging and marking compliance statement
	FICTIONAL DEMONSTRATION SAMPLE. The packhouse, quote, cost, and item data are invented.


Item and packaging source
Solicitation SPE7L0-26-R-DEM4; NSN 4820-01-DEM-0755; Calder CAGE 0DEM7; part CFS-2205-7; drawing revision C; lot CFS-L2606-118; quantity 150 EA.
Juniper Vale Packaging LLC, CAGE 6DEM8, will perform the packaging. Packhouse quote JVP-Q-2026-05-14 prices the required work at $2.20 per unit. Meridian included that amount in the $37.06 landed unit cost used to set the quote price.
Requirement-to-method check
	Solicitation requirement
	Planned method
	Status

	MIL-STD-2073-1E Method 50
	Each capped valve receives the specified barrier and physical protection
	Meets

	Unit pack quantity 1 EA
	One valve per unit container
	Meets

	Manufacturer protective caps remain installed
	Incoming inspection confirmed capped ports; caps stay on through packing
	Meets

	Greaseproof and waterproof barrier
	Barrier applied around each capped valve
	Meets

	Closed-cell cushioning prevents movement
	Cushioning cut to the valve envelope and checked before closure
	Meets

	ASTM D5118 fiberboard unit container
	One labeled fiberboard unit box per valve
	Meets

	Intermediate quantity 10
	Ten unit packs per intermediate container
	Meets

	ASTM D5118 exterior container; palletize as required
	Exterior fiberboard shipper and pallet pattern selected for final quantity
	Meets

	MIL-STD-129R marking
	Award number, NSN, part, CAGE 0DEM7, quantity, unit, and lot printed on required levels
	Meets



The DIBBS quote-form answer is Meets Packaging Requirement: Yes. Final labels receive the award number after award. Lot CFS-L2606-118 appears on the unit, intermediate, and exterior markings so the physical shipment remains tied to the traceability file.
Prepared by: Rana Ellis, Operations Manager Date: 2026-07-10 Signature: /s/ Rana Ellis (FICTIONAL SAMPLE)
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